5639 Benore Road-Toledo, OH 43612

419-727-1100 Toledo

734-782-2480 Flat Rock

**FLAT ROCK/TOLEDO SPEEDWAY RULES AMENDMENTS (MARCH 11, 2024)**

***ARCA FACTORY STOCK/ENDURO CARS***

**Page 45, 1.** Dual overhead cam engines are permitted; Add 50 lbs. for this engine. NO turbo engines.

**Page 47: Weight:** Dual overhead cam engines-2450 lbs. minimum weight.

(The rest of the existing wording in each of these items remains unchanged).

***ARCA LATE MODEL SPORTSMAN CARS***

**Page 42, 16. Weight:** Maximum of 60% left side weight for approved crate engines. Built engines up to 360 CID and built engines over 360 CID maximum left side weight is 60%.

(The rest of the existing wording in this item remains unchanged).

Jack Franzil

Chief Inspector